<!--
notas uteis:
grep -n "^[ ]\+" /home/neo/Público/nfdos/src/Makefile.am
grep -n "^[ ]\+" /home/neo/Público/nfdos/configure.ac
file Makefile.am
file src/Makefile.am
file configure.ac
cat -A Makefile.am | grep '\^I'
cat -A src/Makefile.am | grep '\^I'
cat -A configure.ac | grep '\^I'
nl -ba Makefile | sed -n '770,790p'
grep -n "^[ ]" Makefile | head

grep -E 'X86_PGE|X86_PSE|X86_PSE36|X86_VME|X86_PVI|SMAP|SMEP|RANDOMIZE_BASE|PAGE_TABLE_ISOLATION' src/_nfdos/kernel/linux/.config
grep -E '^CONFIG_CR4' src/_nfdos/kernel/linux/.config || true
---
GRUB:
GRUB_GFXMODE=1024x768x32
GRUB_GFXPAYLOAD_LINUX=keep
-->
"blueprint" do REPL:
```
┌────────────────────────────────────NEURO REPL v0.1───────────────────────────────────────────┐
│ NEUROTRON STATUS   CPU: 2%   MEM: 11%   TEMP: 1.2   ENERGY: 41.0                             │
│ CogState: STABLE   Depth: 1   Valence: -5.00   Mode: ACTIVE                                  │
├──────────────────────────────────────────────────────────────────────────────────────────────┤
│ KERNEL MESSAGES (live):                                                                      │
│ [    0.167890] ACPI: Core revision 20240415                                                  │
│ [    0.260302] pci 0000:00:02.0: VESA 1024x768x32 framebuffer activated                      │
│ [    1.012399] EXT4-fs mounted filesystem with ordered data mode.                            │
│ ...                                                                                          │
├──────────────────────────────────────────────────────────────────────────────────────────────┤
│ NEUROTRON MESSAGES (live):                                                                   │
│ [18:09:04] [info] Neurotron boot() — mode=diagnostic                                         │
│ [18:09:04] [info] Ciclo cognitivo iniciado (observe → think → act → rest)                    │
│ [18:09:04] [disk] Disco detectado: /dev/vda (sem partições visíveis, usando disco inteiro)   │
│ ...                                                                                          │
├──────────────────────────────────────────────────────────────────────────────────────────────┤
│ NEUROTRON CHAT:                                                                              │
│ [ia@nfdos] Olá mundo!                                                                        │
│ [user@nfdos] ...                                                                             │
├──────────────────────────────────────────────────────────────────────────────────────────────┤
│ user@nfdos:                                                                                  │
└──────────────────────────────────────────────────────────────────────────────────────────────┘
```
```
ok a forma geral funcionou. temos um dashboard fixo com o pane status a funcionar:
```
MODE: PERSISTENT  TRM: ACTIVE
CogState: STABLE  Depth: 1  Valence: -2.40  Energy: 7.300

────────────────────────────────────────────────────────────────────────────────
KERNEL MESSAGES (placeholder)







────────────────────────────────────────────────────────────────────────────────
MEMORY MESSAGES (placeholder)







────────────────────────────────────────────────────────────────────────────────
TRM MESSAGES (placeholder)







────────────────────────────────────────────────────────────────────────────────
CHAT MESSAGES (placeholder)[00:48:18] [debug] telemetry state=stable temp=3.7 cpu=16.7% mem=10.6% load=0.14 jitter=0.744s.60 is too large:
[00:48:18] [debug] [trm.explorer] cpu tendência ↑ (+16.7) → energia -0.5ad=0.07 jitter=0.756s3.40 is too large:
[00:48:18] [debug] [trm.thought] Δcpu elevado (+16.7) — reduzir complexidadeepth=1 valence=-2.400. Quota mode: disabled.f
[00:48:18] [debug] [trm.thought] mem estável — tendência favorável.6% load=0.14 jitter=0.764s2.60. Quota mode: disabled.f
[00:48:18] [debug] [trm.thought] sistema frio — margem para explorargy=19.6 depth=1 valence=-2.60mask: ffffffffffffffff
[00:48:18] [debug] [trm.engine] step ok: mode=active cog=stable energy=7.3 depth=1 valence=-2.400mask: ffffffffffffffff
[00:48:18] [heart] cpu=0.0% mem=10.6% tick=0.50stive cog=stable energy=9.3 depth=1 valence=-2.400refined-jiffies' interval of 480030000 ns (480 ms)
[00:47:55] [heart] cpu=0.0% mem=10.6% tick=0.50stive cog=stable energy=40.6 depth=1 valence=-3.60refined-jiffies' interval of 480030000 ns (480 ms)
[00:47:44] [debug] [trm.engine] step ok: mode=active cog=stable energy=43.4 depth=1 valence=-3.60
clocksource:                       'tsc' is current clocksource.
tsc: Marking TSC unstable due to clocksource watchdog
tsc: Marking TSC unstable due to clocksource watchdog
TSC found unstable after boot, most likely due to broken BIOS. Use 'tsc=unstable'.
TSC found unstable after boot, most likely due to broken BIOS. Use 'tsc=unstable'.
sched_clock: Marking unstable (3566043715, 47405219)<-(3626634341, -13185437)
sched_clock: Marking unstable (3566043715, 47405219)<-(3626634341, -13185437)
clocksource: Not enough CPUs to check clocksource 'tsc'.
clocksource: Not enough CPUs to check clocksource 'tsc'.
clocksource: Switched to clocksource refined-jiffies
clocksource: Switched to clocksource refined-jiffies
```
agora temos de ajustar onde as mensagens aparecem nos outros panes, ou como falaste e bem ... definir a API mínima de cada pane