FSCK_OPT=-yf

if [ "$QUOTA" != "y" ]; then
	echo "$test_name: $test_description: skipped"
	return 0
fi

$MKE2FS -q -F -o Linux -I 256 -b 4096 $TMPFILE 10000 > $test_name.log 2>&1
status=$?
if [ "$status" != 0 ] ; then
	echo "mke2fs failed" > $test_name.failed
	echo "$test_name: $test_description: failed"
	return $status
fi

dd if=/dev/zero of=$TMPFILE.2 bs=1048576 count=1 >> $test_name.log 2>&1
cat <<- EOF | $DEBUGFS -w $TMPFILE >> $test_name.log 2>&1
	write $TMPFILE.2 file1
	set_inode_field file1 projid 500
EOF
rm -f $TMPFILE.2

$TUNE2FS -O project $TMPFILE >> $test_name.log 2>&1
status=$?
if [ "$status" != 0 ] ; then
	echo "tune2fs -O project failed with $status" > $test_name.failed
	echo "$test_name: $test_description: failed"
	return $status
fi

$FSCK $FSCK_OPT $TMPFILE >> $test_name.log 2>&1
status=$?
if [ "$status" = 0 ] ; then
	echo "$test_name: $test_description: ok"
	touch $test_name.ok
else
	echo "e2fsck with project enabled failed with $status" > $test_name.failed
	echo "$test_name: $test_description: failed"
	return $status
fi
rm -f $TMPFILE
